{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":7,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-A8"]
[]
[]
[]
[]
["","","","","","2MXM50A2V1B8","2MXM68A2V1B8"]
["Dimenzije","Uređaj","","Visina","mm","552","734"]
["","","","Širina","mm","852","974"]
["","","","Dubina","mm","350","408"]
["Težina","Uređaj","","","kg","41","60"]
["Kompresor","Tip","","","","Hermetički zabrtvljen kompresor s klatnom","Hermetički zabrtvljen kompresor s klatnom"]
["Raspon rada","Hlađenje","Ambijent:","Min.","°C DB","-10","-10"]
["","","","Maks.","°C DB","50","50"]
["Razina tlaka zvuka","Hlađenje","","Nom.","dBA","48","48"]
["","Grijanje","","Nom.","dBA","50","48"]
["Radna tvar","Tip","","","","R-32","R-32"]
["","Punjenje","","","kg","1.15","2.00"]
["","Punjenje","","","tCO2Eq","0.78","1.35"]
["","GWP","","","","675","675"]
["Priključci cjevovoda ","Duljina cjevovoda ","Maks. ","OU - IU","m","20 (1)","25 (1)"]
["Priključci cjevovoda","Punjenje dodatne radne tvari","","","kg/m","002 (za duljinu cjevovoda koja premašuje 20m)","002 (za duljinu cjevovoda koja premašuje 30 m)"]
["","Razlika razine","IU - OU","Maks.","m","15","15"]
["","","IU - IU","Maks.","m","7.5","7.5"]
["","Ukupna duljina cjevovoda","Sustav","Stvarno","m","30","50"]
["Standardna dodatna oprema","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Raspon energetske učinkovitosti","","","","","A+++ ~ D","A+++ ~ D"]
["Napajanje","Faza","","","","1~","1~"]
["","Frekvencija","","","Hz","50","50"]
["","Napon","","","V","220-240","220-240"]
["Napomene","","","","","(1) - Za jednu prostoriju","(1) - Za jednu prostoriju"]
["","","","","","(2) - Za kombinaciju s CVXM-A, FVXM-A - maksimalna duljina cjevovoda je 30 m.","(2) - Za kombinaciju s CVXM-A, FVXM-A - maksimalna duljina cjevovoda je 30 m."]
["","","","","","(3) - Pogledajte odvojene nacrte za radno područje","(3) - Pogledajte odvojene nacrte za radno područje"]
["","","","","","(4) - Vidi električne podatke na posebnim nacrtima","(4) - Vidi električne podatke na posebnim nacrtima"]
["","","","","","(5) - Sadrži fluorovodične stakleničke plinove","(5) - Sadrži fluorovodične stakleničke plinove"]
["Standardna dodatna oprema","Drain cap","","","","","3"]