{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":8,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-N"]
[]
[]
[]
[]
["","","","","","2MXM40N2V1B","2MXM50N2V1B","2MXM68N2V1B"]
["Dimenzije","Uređaj","","Visina","mm","550","550","734"]
["","","","Širina","mm","765","765","958"]
["","","","Dubina","mm","285","285","340"]
["Težina","Uređaj","","","kg","36","41","60"]
["Motor ventilatora","Brzina","Hlađenje","Super nisko","o/min","500","500","420"]
["","","Grijanje","Super nisko","o/min","320","500","420"]
["Kompresor","Type","","","","Hermetički zabrtvljen kompresor s klatnom","Hermetički zabrtvljen kompresor s klatnom","Hermetički zabrtvljen kompresor s klatnom"]
["Raspon rada","Hlađenje","Ambijent:","Min.","°CDB","","","-10"]
["","","","Maks.","°CDB","","","46"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","46","48"]
["","","","Nom.","dBA","","","48"]
["","Grijanje","","Visoko","dBA","48","50"]
["","","","Nom.","dBA","","","48.0"]
["Radna tvar","Tip","","","","R-32","R-32","R-32"]
["","Punjenje","","","kg","0.88","1.15","2"]
["","Punjenje","","","tCO2Eq","0.60","0.78","1.35"]
["","GWP","","","","675","675","675.0"]
["Priključci cjevovoda ","Duljina cjevovoda ","Maks. ","OU - IU","m","20","20","25"]
["Priključci cjevovoda","Punjenje dodatne radne tvari","","","kg/m","0,02 (za duljinu cjevovoda koja premašuje 20m)","0,02 (za duljinu cjevovoda koja premašuje 20m)","0,02 (za duljinu cjevovoda koja premašuje 30 m)"]
["","Razlika razine","IU - OU","Maks.","m","15.0","15.0","15.0"]
["","","IU - IU","Maks.","m","7.5","7.5","7.5"]
["","Ukupna duljina cjevovoda","Sustav","Stvarno","m","30","30","50"]
["Standardna dodatna oprema","Installation manual","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Napajanje","Faza","","","","1~","1~","1~"]
["","Frekvencija","","","Hz","50","50","50"]
["","Napon","","","V","220-230-240","220-230-240","220-240"]
["Napomene","","","","","(1) - Za jednu prostoriju","(1) - Za jednu prostoriju","(1) - Za jednu prostoriju"]
["Standardna dodatna oprema","Reducer assembly","","","","","1","1"]
["","Drain cap","","","","","","3"]