{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXM-A"]
[]
[]
[]
[]
["","","","","","4MXM68A2V1B","4MXM80A2V1B"]
["Dimenzije","Uređaj","","Visina","mm","734","734"]
["","","","Širina","mm","974","974"]
["","","","Dubina","mm","408","408"]
["Težina","Uređaj","","","kg","63","67"]
["Kompresor","Tip","","","","Hermetički zabrtvljen kompresor s klatnom","Hermetički zabrtvljen kompresor s klatnom"]
["Raspon rada","Hlađenje","Ambijent:","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","46","46"]
["Razina tlaka zvuka","Hlađenje","","Nom.","dBA","48","48"]
["","Grijanje","","Nom.","dBA","49","49"]
["Radna tvar","Tip","","","","R-32","R-32"]
["","Punjenje","","","kg","2","2.4"]
["","Punjenje","","","tCO2Eq","1.35","1.62"]
["","GWP","","","","675","675"]
["Priključci cjevovoda ","Duljina cjevovoda ","Maks. ","OU - IU","m","25 (1)","25 (1)"]
["Priključci cjevovoda","Punjenje dodatne radne tvari","","","kg/m","0,02 (za duljinu cjevovoda koja premašuje 30 m)","0,02 (za duljinu cjevovoda koja premašuje 30 m)"]
["","Razlika razine","IU - OU","Maks.","m","15","15"]
["","","IU - IU","Maks.","m","7.5","7.5"]
["","Ukupna duljina cjevovoda","Sustav","Stvarno","m","60","70"]
["Standardna dodatna oprema","Priručnik za instalaciju","","","","1","1"]
["","Drenažni poklopac","","","","3","3"]
["","Drenažni čep","","","","1","1"]
["","Sklop reduktora","","","","1","1"]
["","Vreća s vijcima","","","","1","1"]
["Raspon energetske učinkovitosti","","","","","A+++ ~ D","A+++ ~ D"]
["Napajanje","Faza","","","","1~","1~"]
["","Frekvencija","","","Hz","50","50"]
["","Napon","","","V","220-240","220-240"]
["Napomene","","","","","(1) - Za jednu prostoriju","(1) - Za jednu prostoriju"]
["","","","","","(2) - Pogledajte odvojene nacrte za radno područje","(2) - Pogledajte odvojene nacrte za radno područje"]
["","","","","","(3) - Vidi električne podatke na posebnim nacrtima","(3) - Vidi električne podatke na posebnim nacrtima"]
["","","","","","(4) - Sadrži fluorovodične stakleničke plinove","(4) - Sadrži fluorovodične stakleničke plinove"]