{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":7,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A / AZAS-MV1"]
[]
[]
[]
[]
["","","","","ADEA71A2VEB / AZAS71M2V1B (Archived)","ADEA100A2VEB / AZAS100M7V1B (Archived)","ADEA125A2VEB / AZAS125M7V1B (Archived)"]
["Outdoor unit","","","","AZAS71M2V1B","AZAS100M7V1B","AZAS125M7V1B"]
["Učin hlađenja","Nom.","","kW","6.8","9.5","12.1"]
["Učin grijanja","Nom.","","kW","7.5","10.8","13.5"]
["Nazivna učinkovitost","EER","","","3.27","3.2","2.27"]
["","COP","","","3.62","4.63","3.89"]
["Hlađenje prostora","Razred energetske učinkovitosti","","","A","A"]
["","Kapacitet","Pdesign","kW","6.8","9.5","12.1"]
["","SEER","","","5.44","5.13","4.73"]
["","Godišnja potrošnja energije","","kWh/a","437","648","1,534"]
["Grijanje prostora (prosječna klima)","Razred energetske učinkovitosti","","","A","A"]
["","Kapacitet","Pdesign","kW","4.5","6.0","6.0"]
["","SCOP/A","","","3.81","3.81","3.5"]
["","Pdh kapacitet grijanja pri -10°","","kW","4.5","6.0","6.0"]
["","Godišnja potrošnja energije","","kWh/a","1,654","2,206","2,399"]