{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-A / AZQS-BY1"]
[]
[]
[]
[]
["","","","","ADEQ100A7VEB / AZQS100B7Y1B","ADEQ125A7VE1B / AZQS125B7Y1B"]
["Učin hlađenja","Nom.","","kW","9.5","12.1 (3)"]
["Hlađenje prostora","SEER","","","4.81"]
["","Godišnja potrošnja energije","","kWh/a","692"]
["","Kapacitet","Pdesign","kW","9.50"]
["","Razred energetske učinkovitosti","","","B"]
["Grijanje prostora (prosječna klima)","Kapacitet","Pdesign","kW","7.60"]
["","SCOP/A","","","3.81"]
["","Razred energetske učinkovitosti","","","A"]
["","Godišnja potrošnja energije","","kWh/a","2,793"]
["Nazivna učinkovitost","Godišnja potrošnja energije","","kWh","1,480","2,010"]
["","EER","","","3.21","3.01"]
["","COP","","","3.61","3.45"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","A","B"]
["","","Grijanje","","A","B"]
["Kapacitet grijanja","Nom.","","kW","10.8","13.5 (4)"]
["Napomene","","","","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU"]
["","","","","(2) - Nazivna učinkovitost: hlađenje na 35°/27° nazivnog opterećenja, grijanje na 7°/20° nazivnog opterećenja","(2) - Nazivna učinkovitost: hlađenje na 35°/27° nazivnog opterećenja, grijanje na 7°/20° nazivnog opterećenja"]