{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B"]
[]
[]
[]
[]
["","","","","","FAA71BUV1B","FAA100BUV1B"]
["Kućište","Boja","","","","Bijelo","Bijelo"]
["","Materijal","","","","Smola","Smola"]
["Dimenzije","Uređaj","","Visina","mm","290","340"]
["","","","Širina","mm","1050","1200"]
["","","","Dubina","mm","269","262"]
["Težina","Uređaj","","","kg","14","18"]
["Ventilator","Količina zraka","Hlađenje","Visoko","m³/min","16.2","23"]
["","Protok zraka","Hlađenje","Srednji","m³/min","13.4","21.1"]
["","","","Nizak","m³/min","12.1","18.7"]
["","","Grijanje","Visoko","m³/min","16.9","23"]
["","Protok zraka","Grijanje","Srednji","m³/min","14.2","20.9"]
["","","Grijanje","Nizak","m³/min","12.7","18.7"]
["Zvučna snaga","Hlađenje","","","dBA","61","65"]
["","Grijanje","","","dBA","61","65"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","45","49"]
["Razina zvučnog tlaka","Hlađenje","","Srednji","dBA","42","45"]
["Razina tlaka zvuka","Hlađenje","","Nizak","dBA","40","41"]
["","Grijanje","","Visoko","dBA","45","49"]
["Razina zvučnog tlaka","Grijanje","","Srednji","dBA","42","45"]
["Razina tlaka zvuka","Grijanje","","Nizak","dBA","40","41"]
["Priključci cjevovoda","Tekućina","","VP","mm","9.52","9.52"]
["","Plin","","VP","mm","15.9","15.9"]
["","Odvod vode","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Napajanje","Faza","","","","1~","1~"]
["","Frekvencija","","","Hz","50","50"]
["","Napon","","","V","220-240","220-240"]
["Standardna dodatna oprema","Installation plate","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","4","4"]
["","Heat insulating tape","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["","Screw bag","","","","1","1"]
["Napomene","","","","","(1) - Nom. kapacitet hlađenja se temelji se na sljedećim parametrima: unutarnja temperatura: 27 °C DB, 19 °C WB, vanjska temperatura: 35 °C DB, odgovarajuće cijevi rashladnog sredstva: 5 m, razlika u visini: 0m."]
["","","","","","(2) - Nazivni učin grijanja zasnovani su na: unutarnja temperatura: 20°C DB, vanjska temperatura : 7°C DB, 6°C WB, odgovarajući cjevovod za radnu tvar: 5 m, razlika razine: 0 m."]
["Standardna dodatna oprema","Screw cover","","","","","3"]