{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":9,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FAQ100CVEB / RZQG71L8Y1B","FAQ71CVEB / RZQG71L8Y1B","FAQ100CVEB / RZQG100L8Y1B","FAQ71CVEB / FAQ71CVEB / RZQG100L8Y1B","FAQ71CVEB / FAQ71CVEB / RZQG125L8Y1B"]
["Učin hlađenja","Nom.","","kW","","6.8","9.5"]
["Hlađenje prostora","SEER","","","6.51","6.51","6.11","5.10","5.10"]
["","Godišnja potrošnja energije","","kWh/a","366","366","545","652","824"]
["","Kapacitet","Pdesign","kW","6.80","6.8","9.5","9.50","12.00"]
["","Razred energetske učinkovitosti","","","A++","A++","A++","B","B"]
["Grijanje prostora (prosječna klima)","Kapacitet","Pdesign","kW","6.33","6.33","10.2","11.30","12.71"]
["","SCOP/A","","","4.02","4.02","4.01","3.80","3.80"]
["","Razred energetske učinkovitosti","","","A+","A+","A+","A","A"]
["","Godišnja potrošnja energije","","kWh/a","2,205","2,205","3,562","4,164","4,683"]
["Nazivna učinkovitost","Godišnja potrošnja energije","","kWh","","1,000","1,315"]
["","EER","","","","3.40","3.62"]
["","COP","","","","3.70","3.61"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","","A","A"]
["","","Grijanje","","","A","A"]
["Učin grijanja","Nom.","","kW","","7.5","10.8"]
["Napomene","","","","","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU"]
["","","","","","(2) - Nazivna učinkovitost: hlađenje na 35°/27° nazivnog opterećenja, grijanje na 7°/20° nazivnog opterećenja","(2) - Nazivna učinkovitost: hlađenje na 35°/27° nazivnog opterećenja, grijanje na 7°/20° nazivnog opterećenja"]