{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C9 / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FAQ71CVEB9 / RZQSG71L3V1B","FAQ100CVEB9 / RZQSG100L9V1B"]
["Učin hlađenja","Nom.","","kW","6.8","9.5"]
["Hlađenje prostora","SEER","","","5.81","5.61"]
["","Godišnja potrošnja energije","","kWh/a","410","593"]
["","Kapacitet","Pdesign","kW","6.8","9.50"]
["","Razred energetske učinkovitosti","","","A+","A+"]
["Grijanje prostora (prosječna klima)","Kapacitet","Pdesign","kW","6.33","6.81"]
["","SCOP/A","","","3.90","4.01"]
["","Razred energetske učinkovitosti","","","A","A+"]
["","Godišnja potrošnja energije","","kWh/a","2,273","2,378"]
["Nazivna učinkovitost","Godišnja potrošnja energije","","kWh","1,059","1,580"]
["","EER","","","3.21","3.01"]
["","COP","","","3.61","3.41"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","A","B"]
["","","Grijanje","","A","B"]
["Kapacitet grijanja","Nom.","","kW","7.5","10.8"]
["Napomene","","","","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU"]
["","","","","(2) - Nazivna učinkovitost: hlađenje na 35°/27° nazivnog opterećenja, grijanje na 7°/20° nazivnog opterećenja","(2) - Nazivna učinkovitost: hlađenje na 35°/27° nazivnog opterećenja, grijanje na 7°/20° nazivnog opterećenja"]