{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":12,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FBA35A2VEB / FBA35A2VEB / RZQSG71L3V1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZQSG100L9V1B","FBA50A2VEB / FBA50A2VEB / RZQSG100L9V1B","FBA50A2VEB / FBA50A2VEB / FBA50A2VEB / RZQSG125L9V1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZQSG125L9V1B","FBA60A2VEB / FBA60A2VEB / RZQSG125L9V1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZQSG140L9V1B","FBA71A2VEB / RZQSG71L3V1B"]
["Hlađenje prostora","SEER","","","5.10","5.10","5.10","4.80","4.80","4.80","","5.84"]
["","Godišnja potrošnja energije","","kWh/a","467","652","652","875","875","875","","408"]
["","Kapacitet","Pdesign","kW","6.80","9.50","9.50","12.0","12.0","12.0","","6.80"]
["","Razred energetske učinkovitosti","","","A","A","A","B","B","B","","A+"]
["Grijanje prostora (prosječna klima)","Kapacitet","Pdesign","kW","6.00","7.60","7.60","7.60","7.60","7.60","","6.00"]
["","SCOP/A","","","3.80","3.80","3.80","3.80","3.80","3.80","","4.01"]
["","Razred energetske učinkovitosti","","","A","A","A","A","A","A","","A+"]
["","Godišnja potrošnja energije","","kWh/a","2,211","2,800","2,800","2,800","2,800","2,800","","2,095"]
["Napomene","","","","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 7,5 m; razlika razine: 0 m","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 7,5 m; razlika razine: 0 m","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 7,5 m; razlika razine: 0 m","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 7,5 m; razlika razine: 0 m","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 7,5 m; razlika razine: 0 m","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 7,5 m; razlika razine: 0 m","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 7,5 m; razlika razine: 0 m","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 7,5 m; razlika razine: 0 m"]
["","","","","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m"]
["","","","","(3) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(3) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(3) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(3) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(3) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(3) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(3) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(3) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU"]
["Učin hlađenja","Nom.","","kW","","","9.50 (1)","12.0 (1)","12.0 (1)","12.0 (1)","13.4 (1)","6.80 (1)"]
["Nazivna učinkovitost","EER","","","","","3.06 (3)","2.94 (3)","3.04 (3)","2.83 (3)","4.20 (3)","3.43 (3)"]
["","COP","","","","","3.30 (3)","3.30 (3)","3.35 (3)","3.26 (3)","","3.92 (3)"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","","","B","C","B","C","","A"]
["","","Grijanje","","","","C","C","C","C","","A"]
["Kapacitet grijanja","Nom.","","kW","","","10.8 (2)","13.5 (2)","13.5 (2)","13.5 (2)","15.5 (2)","7.50 (2)"]
["Nazivna učinkovitost","Godišnja potrošnja energije","","kWh","","","","","","","","991"]