{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":21,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAG100AVEB / RZQG71L8Y1B","FCAG100AVEB / RZQG100L8Y1B","FCAG125AVEB / RZQG125L8Y1B","FCAG140AVEB / RZQG100L8Y1B","FCAG140AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG100L8Y1B","FCAG50AVEB / FCAG50AVEB / RZQG100L8Y1B","FCAG50AVEB / FCAG50AVEB / FCAG50AVEB / RZQG125L8Y1B","FCAG60AVEB / FCAG60AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / RZQG71L8Y1B","FCAG50AVEB / FCAG50AVEB / RZQG71L8Y1B","FCAG71AVEB / RZQG71L8Y1B","FCAG71AVEB / FCAG71AVEB / RZQG100L8Y1B","FCAG71AVEB / FCAG71AVEB / RZQG125L8Y1B","FCAG140AVEB / RZQG140L7Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG140L7Y1B"]
["Raspon energetske učinkovitosti","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","","","","A+++ ~ D","A+++ ~ D"]
["Hlađenje prostora","SEER","","","","","","","","","","","","","5.10","5.10","6.72","","","6.44","9.70"]
["","Godišnja potrošnja energije","","kWh/a","","","","","","","","","","","467","467","355","","","1,249","829"]
["","Kapacitet","Pdesign","kW","","","","","","","","","","","6.80","6.80","6.80","","","13.4","13.4"]
["","Razred energetske učinkovitosti","","","","","","","","","","","","","A","A","A++"]
["Grijanje prostora (prosječna klima)","Kapacitet","Pdesign","kW","","","","","","","","","","","6.00","6.00","6.33","","","11.6","12.0"]
["","SCOP/A","","","","","","","","","","","","","3.80","3.80","4.20","","","4.27","3.96"]
["","Razred energetske učinkovitosti","","","","","","","","","","","","","A","A","A+"]
["","Godišnja potrošnja energije","","kWh/a","","","","","","","","","","","2,211","2,211","2,110","","","3,795","4,235"]
["Napomene","","","","","","","","","","","","","","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 7,5 m; razlika razine: 0 m","","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 7,5 m; razlika razine: 0 m","","","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 7,5 m; razlika razine: 0 m","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 7,5 m; razlika razine: 0 m"]
["","","","","","","","","","","","","","","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m","","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m","","","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m"]
["","","","","","","","","","","","","","","(3) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","","(3) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","","","(3) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(3) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU"]
["Učin hlađenja","Nom.","","kW","","","","","","","","","","","","","6.80 (1)","","","13.4 (1)","13.4 (1)"]
["Nazivna učinkovitost","Godišnja potrošnja energije","","kWh","","","","","","","","","","","","","1,005"]
["","EER","","","","","","","","","","","","","","","3.39 (3)","","","2.50 (3)","4.29 (3)"]
["","COP","","","","","","","","","","","","","","","3.97 (3)","","","3.61 (3)"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","","","","","","","","","","","","","A"]
["","","Grijanje","","","","","","","","","","","","","","A"]
["Kapacitet grijanja","Nom.","","kW","","","","","","","","","","","","","7.50 (2)","","","15.5 (2)","15.5 (2)"]
["Vanjska jedinica","","","","","","","","","","","","","","","","","RZQG100L8Y1","RZQG125L8Y1"]
["Hlađenje prostora","Razred energetske učinkovitosti","","","","","","","","","","","","","","","","A","A"]
["","Kapacitet","Pdesign","kW","","","","","","","","","","","","","","9.50","12.0"]
["","SEER","","","","","","","","","","","","","","","","5.10","5.10"]
["","Godišnja potrošnja energije","","kWh/a","","","","","","","","","","","","","","652","824"]
["Grijanje prostora (prosječna klima)","Razred energetske učinkovitosti","","","","","","","","","","","","","","","","A","A"]
["","Kapacitet","Pdesign","kW","","","","","","","","","","","","","","11.3","12.7"]
["","SCOP/A","","","","","","","","","","","","","","","","3.80","3.80"]
["","Godišnja potrošnja energije","","kWh/a","","","","","","","","","","","","","","4164","4683"]
["Hlađenje prostora","ηs,c","","%","","","","","","","","","","","","","","","","254.6","385.1"]
["Grijanje prostora (prosječna klima)","ηs,h","","%","","","","","","","","","","","","","","","","167.6","155.2"]