{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":24,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FCAG100AVEB / RZQG71L9V1B","FCAG100AVEB / RZQG100L9V1B","FCAG50AVEB / FCAG50AVEB / FCAG50AVEB / RZQG125L9V1B","FCAG60AVEB / FCAG60AVEB / RZQG125L9V1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG100L9V1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG125L9V1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG100L9V1B","FCAG50AVEB / FCAG50AVEB / FCAG50AVEB / RZQG100L9V1B","FCAG50AVEB / FCAG50AVEB / RZQG100L9V1B","FCAG71AVEB / FCAG71AVEB / RZQG100L9V1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG71L9V1B","FCAG35AVEB / FCAG35AVEB / RZQG71L9V1B","FCAG50AVEB / FCAG50AVEB / RZQG71L9V1B","FCAG71AVEB / RZQG71L9V1B","FCAG140AVEB / RZQG100L9V1B","FCAG125AVEB / RZQG125L9V1B","FCAG140AVEB / RZQG125L9V1B","FCAG71AVEB / FCAG71AVEB / RZQG125L9V1B","FCAG140AVEB / RZQG140L9V1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG140L9V1B"]
["Učin hlađenja","Nom.","","kW","","","","","","","","","","","","","","6.80 (1)","","12.0 (1)","","","13.4 (1)","13.4 (1)"]
["Hlađenje prostora","SEER","","","","","","","","","","","","","5.10","5.10","5.10","6.72","6.80","6.00","6.00","5.10","6.44","9.70"]
["","ηs,c","","%","","","","","","","","","","","","","","","","","","","254.6","385.1"]
["","Godišnja potrošnja energije","","kWh/a","","","","","","","","","","","467","467","467","355","489","700","700","824","1,249","829"]
["","Kapacitet","Pdesign","kW","","","","","","","","","","","6.80","6.80","6.80","6.80","9.50","12.0","12.00","12.0","13.4","13.4"]
["","Razred energetske učinkovitosti","","","","","","","","","","","","","A","A","A","A++","A++","A+","A+","A"]
["Grijanje prostora (prosječna klima)","Kapacitet","Pdesign","kW","","","","","","","","","","","6.00","6.00","6.00","6.33","11.30","12.7","12.66","12.7","11.6","12.0"]
["","SCOP/A","","","","","","","","","","","","","3.80","3.80","3.80","4.20","4.61","4.10","4.10","3.80","4.27","3.96"]
["","Razred energetske učinkovitosti","","","","","","","","","","","","","A","A","A","A+","A++","A+","A+","A"]
["","Godišnja potrošnja energije","","kWh/a","","","","","","","","","","","2,211","2,211","2,211","2,110","3,432","4,323","4,323","4,683","3,795","4,235"]
["","ηs,h","","%","","","","","","","","","","","","","","","","","","","167.6","155.2"]
["Nazivna učinkovitost","Godišnja potrošnja energije","","kWh","","","","","","","","","","","","","","1,005","","1,610"]
["","EER","","","","","","","","","","","","","","","","3.39 (3)","","3.73 (3)","","","2.50 (3)","4.29 (3)"]
["","COP","","","","","","","","","","","","","","","","3.97 (3)","","3.63 (3)","","","3.61 (3)"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","","","","","","","","","","","","","","A","","A"]
["","","Grijanje","","","","","","","","","","","","","","","A","","A"]
["Učin grijanja","Nom.","","kW","","","","","","","","","","","","","","7.50 (2)","","13.5 (2)","","","15.5 (2)","15.5 (2)"]
["Napomene","","","","","","","","","","","","","","","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 7,5 m; razlika razine: 0 m","","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 7,5 m; razlika razine: 0 m","","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 7,5 m; razlika razine: 0 m","","","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 7,5 m; razlika razine: 0 m","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 7,5 m; razlika razine: 0 m"]
["","","","","","","","","","","","","","","","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m","","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m","","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m","","","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m"]
["","","","","","","","","","","","","","","","(3) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","","(3) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","","(3) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","","","(3) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(3) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU"]
["Raspon energetske učinkovitosti","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]