{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":16,"n_cols":5,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / AZQS-BY1 UK"]
[]
[]
[]
[]
["","","","","FCQG125FVEB / AZQS125B7Y1B UK"]
["Učin hlađenja","Nom.","","kW","12.1"]
["Nazivna učinkovitost","Godišnja potrošnja energije","","kWh","1,952"]
["","EER","","","3.10"]
["","COP","","","3.41"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","B"]
["","","Grijanje","","B"]
["Kapacitet grijanja","Nom.","","kW","13.5"]
["Napomene","","","","(1) - Godišnja potrošnja energije u skladu je s direktivom oznake energetske učinkovitosti 2002/31/EC"]
["","","","","(2) - SEER i SCOP su u skladu s EN 14825"]
["","","","","(3) - Nazivna učinkovitost: hlađenje na 35°/27° nazivnog opterećenja, grijanje na 7°/20° nazivnog opterećenja"]