{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":6,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C"]
[]
[]
[]
[]
["","","","","FDQ125C5VEB","FDQ125C7VEB"]
["Nivo zvučnog tlaka","Grijanje","Visoko","dBA","40","40"]
["","","Nizak","dBA","33","33"]
["","Hlađenje","Nizak","dBA","33","33"]
["","","Visoko","dBA","40","40"]
["Upravljački sustavi","Žično daljinsko upravljanje","","","BRC1D52, BRC1E53A, BRC1E53B, BRC1E53C","BRC1D52, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D528"]
["","Infrared remote control","","","BRC4C65","BRC4C65"]
["Učin hlađenja","Ukupni učin","Nom.","kW","12.5 (1)","12.5"]
["Priključci cjevovoda","Tekućina","VP","mm","9.52","9.52"]
["","Plin","VP","mm","15.9","15.9"]
["","Odvod vode","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Ulazna struja","Hlađenje","Nom.","kW","0.35"]
["","Grijanje","Nom.","kW","0.35"]
["Potreban otvor u stropu >","mm","","","350","350"]
["Sound power level","Hlađenje","","dBA","66","66"]
["Dimenzije","Uređaj","Širina","mm","1,400","1,400"]
["","","Depth","mm","700","700"]
["","","Visina","mm","300","300"]
["Kućište","Materijal","","","","Galvanizirani čelik"]
["","Boja","","","Nije obojeno (galvanizirano)","Not painted"]
["Težina","Uređaj","","kg","45","45"]
["Ventilator","Vanjski statički tlak","Visoki","Pa","200","200"]
["","","Nom.","Pa","50","50"]
["Odvod do visine","mm","","","625","625"]
["Dekorativni panel","Težina","","kg","6.5","6.5"]
["","Model","","","BYBS125DJW1","BYBS125DJW1"]
["","Dimenzije","Visina","mm","55","55"]
["","","Dubina","mm","500","500"]
["","","Širina","mm","1,500","1,500"]
["","Boja","","","Bijelo (10Y9/0.5)","Bijelo (10Y9/0.5)"]
["Učin grijanja","Ukupni učin","Nom.","kW","14.0 (2)","14.0"]
["Power supply","Phase","","","1~","1~"]
["","Frekvencija","","Hz","50/60","50/60"]
["","Naziv","","","VE","VE"]
["","Napon","","V","220-240/220","220-240/220"]
["Napomene","","","","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19,0°CWB; vanjska temp. 35°CDB; odgovarajuća duljina cijevi; 7,5 m; razlika u razini: 0 m","(1) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m"]
["","","","","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m","(2) - Učini su neto, uključujući odbitke za hlađenje (dodatke za grijanje) za toplinu motora unutarnjeg ventilatora."]
["","","","","(3) - Učini su neto, uključujući odbitke za hlađenje (dodatke za grijanje) za toplinu motora unutarnjeg ventilatora.","(3) - Vrijednosti tlaka zvuka navedene su za jedinicu instaliranu sa stražnjim usisom."]
["","","","","(4) - Vrijednosti tlaka zvuka navedene su za jedinicu instaliranu sa stražnjim usisom.","(4) - Kategorija PED jedinice: isključeno iz PED opsega zbog članka 1., stavke 3.6 od 97/23/EC"]
["","","","","(5) - Kategorija PED jedinice: isključeno iz PED opsega zbog članka 1., stavke 3.6 od 97/23/EC","(5) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 7,5 m (vodoravno); razlika razine: 0 m"]