{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":9,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / RZQSG100L9V1B","FDXM50F3V1B / FDXM50F3V1B / RZQSG100L9V1B","FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / RZQSG125L9V1B","FDXM50F3V1B / FDXM50F3V1B / FDXM50F3V1B / RZQSG125L9V1B","FDXM60F3V1B / FDXM60F3V1B / RZQSG125L9V1B"]
["Hlađenje prostora","Godišnja potrošnja energije","","kWh/a","693","652","875","875","875"]
["","Kapacitet","Pdesign","kW","9.50","9.50","12.0","12.0","12.0"]
["Grijanje prostora (prosječna klima)","Kapacitet","Pdesign","kW","7.10","7.60","7.60","7.60","7.60"]
["","Godišnja potrošnja energije","","kWh/a","2,616","2,800","2,800","2,800","2,800"]
["Hlađenje prostora","SEER","","","4.80","5.10","4.80","4.80","4.80"]
["","Razred energetske učinkovitosti","","","B","A","B","B","B"]
["Grijanje prostora (prosječna klima)","SCOP/A","","","3.80","3.80","3.80","3.80","3.80"]
["","Razred energetske učinkovitosti","","","A","A","A","A","A"]
["Napomene","","","","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 7,5 m; razlika razine: 0 m","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 7,5 m; razlika razine: 0 m","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 7,5 m; razlika razine: 0 m","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 7,5 m; razlika razine: 0 m","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 7,5 m; razlika razine: 0 m"]
["","","","","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m"]
["","","","","(3) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(3) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(3) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(3) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(3) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU"]