{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RXM-M9"]
[]
[]
[]
[]
["","","","","FHA35AVEB / RXM35M3V1B9","FHA50AVEB / RXM50M3V1B9","FHA60AVEB / RXM60M3V1B9"]
["Učin hlađenja","Nom.","","kW","3.40"]
["Hlađenje prostora","SEER","","","6.24"]
["","Godišnja potrošnja energije","","kWh/a","191"]
["","Kapacitet","Pdesign","kW","3.40"]
["","Razred energetske učinkovitosti","","","A++"]
["Grijanje prostora (prosječna klima)","Kapacitet","Pdesign","kW","3.10"]
["","SCOP/A","","","4.43"]
["","Razred energetske učinkovitosti","","","A+"]
["","Godišnja potrošnja energije","","kWh/a","979"]
["Nazivna učinkovitost","Godišnja potrošnja energije","","kWh","456"]
["","EER","","","3.73"]
["","COP","","","4.08"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","A"]
["","","Grijanje","","A"]
["Kapacitet grijanja","Nom.","","kW","4.00"]
["Napomene","","","","(1) - Vidi električne podatke na posebnim nacrtima"]
["","","","","(2) - Pogledajte odvojene nacrte za radno područje"]
["","","","","(3) - Nom. kapacitet hlađenja se temelji se na sljedećim parametrima: unutarnja temperatura: 27 °C DB, 19 °C WB, vanjska temperatura: 35 °C DB, odgovarajuće cijevi rashladnog sredstva: 5 m, razlika u visini: 0m."]
["","","","","(4) - Nazivni učin grijanja zasnovani su na: unutarnja temperatura: 20°C DB, vanjska temperatura : 7°C DB, 6°C WB, odgovarajući cjevovod za radnu tvar: 5 m, razlika razine: 0 m."]
["Outdoor unit","","","","","RXM50M3V1B9","RXM60M3V1B9"]
["Učin hlađenja","Nom.","","kW","","5.00","5.70"]
["Učin grijanja","Nom.","","kW","","6.00","7.20"]
["Nazivna učinkovitost","EER","","","","3.21","3.29"]
["","COP","","","","3.35","3.32"]
["","Godišnja potrošnja energije","","kWh","","780","867"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","","B","A"]
["","","Grijanje","","","C","C"]
["Hlađenje prostora","Razred energetske učinkovitosti","","","","A+","A+"]
["","Kapacitet","Pdesign","kW","","5.00","5.70"]
["","SEER","","","","5.92","6.08"]
["","Godišnja potrošnja energije","","kWh/a","","295","328"]
["Grijanje prostora (prosječna klima)","Razred energetske učinkovitosti","","","","A","A"]
["","Kapacitet","Pdesign","kW","","4.35","4.71"]
["","SCOP/A","","","","3.86","3.87"]
["","Pdh kapacitet grijanja pri -10°","","kW","","3.85","4.08"]
["","Godišnja potrošnja energije","","kWh/a","","1578","1704"]