{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":16,"n_cols":9,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNQ-A / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FNQ35A2VEB / FNQ35A2VEB / FNQ35A2VEB / RZQSG100L8Y1B","FNQ50A2VEB / FNQ50A2VEB / RZQSG100L8Y1B","FNQ60A2VEB / FNQ60A2VEB / RZQSG125L8Y1B","FNQ35A2VEB / FNQ35A2VEB / FNQ35A2VEB / FNQ35A2VEB / RZQSG125L8Y1B","FNQ50A2VEB / FNQ50A2VEB / FNQ50A2VEB / RZQSG125L8Y1B"]
["Hlađenje prostora","SEER","","","4.80","5.10","4.80","4.80","4.80"]
["","Godišnja potrošnja energije","","kWh/a","693","652","875","875","875"]
["","Kapacitet","Pdesign","kW","9.50","9.50","12.00","12.00","12.00"]
["","Razred energetske učinkovitosti","","","B","A","B","B","B"]
["Grijanje prostora (prosječna klima)","Kapacitet","Pdesign","kW","7.10","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","3.80","3.80","3.80","3.80","3.80"]
["","Razred energetske učinkovitosti","","","A","A","A","A","A"]
["","Godišnja potrošnja energije","","kWh/a","2,616","2,800","2,800","2,800","2,800"]
["Napomene","","","","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU"]
["","","","","(2) - Nazivna učinkovitost: hlađenje na 35°/27° nazivnog opterećenja, grijanje na 7°/20° nazivnog opterećenja","(2) - Nazivna učinkovitost: hlađenje na 35°/27° nazivnog opterećenja, grijanje na 7°/20° nazivnog opterećenja","(2) - Nazivna učinkovitost: hlađenje na 35°/27° nazivnog opterećenja, grijanje na 7°/20° nazivnog opterećenja","(2) - Nazivna učinkovitost: hlađenje na 35°/27° nazivnog opterećenja, grijanje na 7°/20° nazivnog opterećenja","(2) - Nazivna učinkovitost: hlađenje na 35°/27° nazivnog opterećenja, grijanje na 7°/20° nazivnog opterećenja"]