{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":8,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-N9"]
[]
[]
[]
[]
["","","","","","FTXP35N5V1B9","FTXP50N5V1B9","FTXP20N5V1B9 (Archived)"]
["Ulazna struja","Hlađenje","","Nom.","kW","0.032","0.04","0.021"]
["","Grijanje","","Nom.","kW","0.032","0.04","0.023"]
["Kućište","Boja","","","","Bijelo","Bijelo","Bijelo"]
["Dimenzije","Uređaj","","Visina","mm","286","286","286"]
["","","","Širina","mm","770","770","770"]
["","","","Dubina","mm","225","225","225"]
["Težina","Uređaj","","","kg","9","9","9"]
["Ventilator","Količina zraka","Hlađenje","Visoko","m³/min","11.5","11.8","9.6"]
["","Protok zraka","Hlađenje","Srednji","m³/min","8.3","9.3","7.5"]
["","","","Nizak","m³/min","6.3","7.6","5.6"]
["","","","Tihi način rada","m³/min","4.5","6","4.4"]
["","","Grijanje","Visoko","m³/min","11.5","11.9","10.6"]
["","Protok zraka","Grijanje","Srednji","m³/min","9","9.5","8.6"]
["","","Grijanje","Nizak","m³/min","7","8.2","6.6"]
["","","","Tihi način rada","m³/min","5.1","7.4","5"]
["Zvučna snaga","Hlađenje","","","dBA","58","59","55"]
["","Grijanje","","","dBA","58","61","55"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","43","46","39"]
["Razina zvučnog tlaka","Hlađenje","","Srednji","dBA","34","39","33"]
["Razina tlaka zvuka","Hlađenje","","Nizak","dBA","27","34","25"]
["","","","Tihi način rada","dBA","20","27","19"]
["","Grijanje","","Visoko","dBA","40","44","39"]
["Razina zvučnog tlaka","Grijanje","","Srednji","dBA","35","38","34"]
["Razina tlaka zvuka","Grijanje","","Nizak","dBA","29","33","28"]
["","","","Tihi način rada","dBA","21","30","21"]
["Priključci cjevovoda","Tekućina","","VP","mm","6.35","6.35","6.35"]
["","Plin","","VP","mm","9.52","12.7","9.52"]
["","Odvod vode","","","","18","18","18"]
["Upravljački sustavi","Infracrveno daljinsko upravljanje","","","","ARC480A78","ARC480A78","ARC480A78"]
["","Žično daljinsko upravljanje","","","","BRC073A1","BRC073A1","BRC073A1"]
["Standardna dodatna oprema","Installation manual","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1"]
["","Silver particle filter","","","","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2"]
["","Infrared remote control","","","","1","1","1"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Napajanje","Faza","","","","1~","1~","1~"]
["","Frekvencija","","","Hz","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240"]
["Napomene","","","","","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 5 m; razlika razine: 0 m","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 5 m; razlika razine: 0 m","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 5 m; razlika razine: 0 m"]
["","","","","","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 5 m (vodoravno)","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 5 m (vodoravno)","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 5 m (vodoravno)"]
["","","","","","(3) - Vidi električne podatke na posebnim nacrtima","(3) - Vidi električne podatke na posebnim nacrtima","(3) - Vidi električne podatke na posebnim nacrtima"]