{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":15,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K"]
[]
[]
[]
[]
["","","","","","FTXS20K2V1B","FTXS20K3V1B","FTXS25K2V1B","FTXS25K3V1B","FTXS35K2V1B","FTXS35K3V1B","FTXS42K2V1B","FTXS42K3V1B","FTXS50K2V1B","FTXS50K3V1B"]
["Razina tlaka zvuka","Grijanje","","Visoko","dBA","40","","","","","","45"]
["","","","Tihi način rada","dBA","19","","","","","","22"]
["","","","Nizak","dBA","27","","","","","","33"]
["","Hlađenje","","Tihi način rada","dBA","19","","","","","","21"]
["","","","Nizak","dBA","24","","","","","","33"]
["","","","Visoko","dBA","40","","","","","","45"]
["","","","Nom.","dBA","34","","","","","","39"]
["","Hlađenje","","Nom.","dBA","32","","","","","","39"]
["Standardna dodatna oprema","Priručnik za instalaciju","","","","1","","","","","","1"]
["","Radni priručnik","","","","1","","","","","","1"]
["","Bežični daljinski upravljač","","","","1","","","","","","1"]
["","Baterije","","","","2","","","","","","2"]
["","Držač daljinskog upravljača","","","","1","","","","","","1"]
["","Montažna ploča","","","","1","","","","","","1"]
["","Učvrsni vijak unutarnje jedinice","","","","2","","","","","","2"]
["","Fotokatalitički filtar za pročišćavanje zraka iz titan-apatita","","","","2","","","","","","2"]
["Upravljački sustavi","Infrared remote control","","","","ARC466A6","","","","","","ARC466A6"]
["Priključci cjevovoda","Tekućina","","VP","mm","6.35","","","","","","6.35"]
["","Plin","","VP","mm","9.5","","","","","","9.5"]
["","Odvod vode","","","","18","","","","","","18"]
["Ulazna struja","Hlađenje","","Nom.","kW","0.04","","","","","","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Grijanje","","Nom.","kW","0.04","","","","","","0.030 (2), 0.030 (3), 0.030 (4)"]
["Sound power level","Hlađenje","","","dBA","58","","","","","","59"]
["","Grijanje","","","dBA","58","","","","","","59"]
["Dimenzije","Uređaj","","Širina","mm","780","","","","","","900"]
["","","","Dubina","mm","215","","","","","","215"]
["","","","Visina","mm","289","","","","","","298"]
["Kućište","Boja","","","","Bijelo","","","","","","Bijelo"]
["Težina","Uređaj","","","kg","8","","","","","","11"]
["Power supply","Faza","","","","1~","","","","","","1~"]
["","Frekvencija","","","Hz","50","","","","","","50"]
["","Naziv","","","","V1","","","","","","V1"]
["","Napon","","","V","220-240","","","","","","220-240"]
["Napomene","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - Kada se spaja s vanjskom jedinicom za više sustava, pogledajte tehničke podatke vanjske jedinice za više sustava koju treba spojiti.","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 220 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 230 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["Ulazna struja","Hlađenje","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (3) (1) (2), 0.040 (3) (1) (2), 0.040 (3) (1) (2)","0.026 (3) (4) (2), 0.026 (3) (4) (2), 0.026 (3) (4) (2)","0.026 (1) (3) (2), 0.026 (1) (3) (2), 0.026 (1) (3) (2)","","0.024, 0.024, 0.024","0.026 (4) (2) (3), 0.026 (4) (2) (3), 0.026 (4) (2) (3)","0.026 (1) (2) (3), 0.026 (1) (2) (3), 0.026 (1) (2) (3)"]
["","Grijanje","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)","0.028 (2) (4) (3), 0.028 (2) (4) (3), 0.028 (2) (4) (3)","0.028 (1) (3) (2), 0.028 (1) (3) (2), 0.028 (1) (3) (2)","","0.030, 0.030, 0.030","0.032 (2) (4) (3), 0.032 (2) (4) (3), 0.032 (2) (4) (3)","0.032 (2) (1) (3), 0.032 (2) (1) (3), 0.032 (2) (1) (3)"]
["Kućište","Boja","","","","","Bijelo","Bijelo","Bijelo","Bijelo","Bijelo","","Bijelo","Bijelo","Bijelo"]
["Dimenzije","Uređaj","","Visina","mm","","215","289","215","298","215","","215","298","215"]
["","","","Širina","mm","","780","780","780","900","900","","900","900","900"]
["","","","Dubina","mm","","289","215","289","215","298","","298","215","298"]
["Težina","Uređaj","","","kg","","8.00","8","8.00","11","11.0","","11.0","11","11.0"]
["Ventilator","Količina zraka","Hlađenje","Visoko","m³/min","","8.8","9.1","9.1","11.2","11.2","","11.2","11.9","11.9"]
["","Protok zraka","Hlađenje","Srednji","m³/min","","6.7","7.0","7.0","","8.5","","9.1","","9.6"]
["","","","Nizak","m³/min","","4.7","5.0","5.0","5.8","5.8","","7.0","7.4","7.4"]
["","","","Tihi način rada","m³/min","","3.9","3.9","3.9","4.1","4.1","","4.1","4.5","4.5"]
["","","Grijanje","Visoko","m³/min","","9.5","10.0","10.0","12.1","12.1","","12.4","13.3","13.3"]
["","Protok zraka","Grijanje","Srednji","m³/min","","7.8","8.0","8.0","","9.3","","10.0","","10.8"]
["","","Grijanje","Nizak","m³/min","","6.0","6.0","6.0","6.5","6.5","","7.8","8.4","8.4"]
["","","","Tihi način rada","m³/min","","4.3","4.3","4.3","4.2","4.2","","5.2","5.5","5.5"]
["Zvučna snaga","Hlađenje","","","dBA","","58","58","58","59","59","","59","60","60"]
["","Grijanje","","","dBA","","58","58","58","59","59","","59","60","60"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","","40","41","41","45","45","","45","46","46"]
["Razina zvučnog tlaka","Hlađenje","","Srednji","dBA","","32","33","33","","37","","39","","40"]
["Razina tlaka zvuka","Hlađenje","","Nizak","dBA","","24","25","25","29","29","","33","34","34"]
["","","","Tihi način rada","dBA","","19","19","19","19","19","","21","23","23"]
["","Grijanje","","Visoko","dBA","","40","41","41","45","45","","45","47","47"]
["Razina zvučnog tlaka","Grijanje","","Srednji","dBA","","34","34","34","","39","","39","","40"]
["Razina tlaka zvuka","Grijanje","","Nizak","dBA","","27","27","27","29","29","","33","34","34"]
["","","","Tihi način rada","dBA","","19","19","19","19","19","","22","24","24"]
["Priključci cjevovoda","Tekućina","","VP","mm","","6.35","6.35","6.35","6.35","6.35","","6.35","6.35","6.35"]
["","Plin","","VP","mm","","9.50","9.5","9.50","9.5","9.50","","9.50","12.7","12.7"]
["","Odvod vode","","","","","18","18","18","18","18","","18","18","18"]
["Upravljački sustavi","Infrared remote control","","","","","ARC466A6","","","","","","ARC466A9"]
["Standardna dodatna oprema","Installation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","","2","","2","","2","","2"]
["","Operation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2","","2","","2","","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","","1","1","1"]
["Napajanje","Naziv","","","","","V1","V1","V1","V1","V1","","V1","V1","V1"]
["","Faza","","","","","1~","1~","1~","1~","1~","","1~","1~","1~"]
["","Frekvencija","","","Hz","","50","50","50","50","50","","50","50","50"]
["","Napon","","","V","","220-240","220-240","220-240","220-240","220-240","","220-240","220-240","220-240"]
["Ventilator","Količina zraka","Hlađenje","Nom.","m³/min","","","9.1","","11.2","","","","11.9"]
["Razina tlaka zvuka","Hlađenje","","Nom.","dBA","","","33","","37","","","","40"]
["Ventilator","Količina zraka","Grijanje","Nom.","m³/min","","","8.0","","9.3","","","","10.8"]
["Razina tlaka zvuka","Grijanje","","Nom.","dBA","","","34","","39","","","","40"]
["Upravljački sustavi","Infracrveno daljinsko upravljanje","","","","","","ARC466A6","ARC466A6","ARC466A6","ARC466A9","","","ARC466A6","ARC466A9"]
["Standardna dodatna oprema","Batteries","","","","","","2","","2","","","","2"]
["","Titanium apatite photocatalytic air purification filter","","","","","","2","","2","","","","2"]
["Napomene","","","","","","","","","","","(4) - 240 V"]