{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":94,"n_cols":7,"rows_kept":94,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-R"]
[]
[]
[]
[]
["","","","","","FTXTM30R2V1B","FTXTM40R2V1B"]
["Razina tlaka zvuka","Grijanje","","Visoko","dBA","45.0"]
["","","","Srednji","dBA","31.0"]
["","","","Tihi način rada","dBA","19.0"]
["","","","Nizak","dBA","22.0"]
["","Hlađenje","","Srednji","dBA","33.0"]
["","","","Tihi način rada","dBA","21.0"]
["","","","Nizak","dBA","25.0"]
["","","","Visoko","dBA","45.0"]
["Standardna dodatna oprema","Priručnik za instalaciju","","","","1"]
["","Radni priručnik","","","","1"]
["","Bežični daljinski upravljač","","","","1"]
["","AAA suhe baterije","","","","2"]
["","Držač daljinskog upravljača","","","","1"]
["","Montažna ploča","","","","1"]
["","Učvrsni vijak unutarnje jedinice","","","","2"]
["","Srebrni filter","","","","1"]
["Upravljački sustavi","Wired remote control","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A75"]
["Priključci cjevovoda","Tekućina","","VP","mm","6.35"]
["","Plin","","VP","mm","9.50"]
["","Odvod vode","","","","18"]
["Priključna snaga","Hlađenje","","Nom.","kW","0.035"]
["","Grijanje","","Nom.","kW","0.039"]
["Sound power level","Hlađenje","","","dBA","60.0"]
["","Grijanje","","","dBA","61.0"]
["Dimenzije","Uređaj","","Širina","mm","778"]
["","","","Dubina","mm","272"]
["","","","Visina","mm","295"]
["Casing","Colour","","","","Bijelo"]
["Težina","Uređaj","","","kg","10.0"]
["Fan","Količina zraka","Grijanje","Visoko","m³/min","12.5"]
["","","","Nizak","m³/min","4.9"]
["","","","Srednji","m³/min","7.5"]
["","","","Tihi način rada","m³/min","4.0"]
["","","Hlađenje","Nizak","m³/min","5.3"]
["","","","Srednji","m³/min","7.8"]
["","","","Visoko","m³/min","12.2"]
["","","","Tihi način rada","m³/min","4.1"]
["Power supply","Phase","","","","1~"]
["","Frekvencija","","","Hz","50"]
["","Naziv","","","","V1"]
["","Napon","","","V","220-240"]
["Napomene","","","","","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19,0°CWB; vanjska temperatura 35°CDB; 24°CWB, duljina odgovarajućeg cjevovoda: 5 m"]
["","","","","","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 5 m"]
["","","","","","(3) - Vidi električne podatke na posebnim nacrtima"]
["Ulazna struja","Hlađenje","","Nom.","kW","","0.053"]
["","Grijanje","","Nom.","kW","","0.06"]
["Kućište","Boja","","","","","Bijelo"]
["Dimenzije","Uređaj","","Visina","mm","","299"]
["","","","Širina","mm","","998"]
["","","","Dubina","mm","","292"]
["Težina","Uređaj","","","kg","","14.5"]
["Ventilator","Količina zraka","Hlađenje","Visoko","m³/min","","15.4"]
["","Protok zraka","Hlađenje","Srednji","m³/min","","9.5"]
["","","","Nizak","m³/min","","5.8"]
["","","","Tihi način rada","m³/min","","4.6"]
["","","Grijanje","Visoko","m³/min","","17.5"]
["","Protok zraka","Grijanje","Srednji","m³/min","","10.5"]
["","","Grijanje","Nizak","m³/min","","7.1"]
["","","","Tihi način rada","m³/min","","5.9"]
["Zvučna snaga","Hlađenje","","","dBA","","60"]
["","Grijanje","","","dBA","","61"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","","46"]
["Razina zvučnog tlaka","Hlađenje","","Srednji","dBA","","32"]
["Razina tlaka zvuka","Hlađenje","","Nizak","dBA","","24"]
["","","","Tihi način rada","dBA","","20"]
["","Grijanje","","Visoko","dBA","","46"]
["Razina zvučnog tlaka","Grijanje","","Srednji","dBA","","31"]
["Razina tlaka zvuka","Grijanje","","Nizak","dBA","","22"]
["","","","Tihi način rada","dBA","","19"]
["Priključci cjevovoda","Tekućina","","VP","mm","","6.35"]
["","Plin","","VP","mm","","9.5"]
["","Odvod vode","","","","","18"]
["Upravljački sustavi","Infrared remote control","","","","","ARC466A75"]
["Upravljački sustavi","Žično daljinsko upravljanje","","","","","BRC073A1"]
["Standardna dodatna oprema","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","1"]
["","Silver particle filter","","","","","1"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Napajanje","Naziv","","","","","V1"]
["","Faza","","","","","1~"]
["","Frekvencija","","","Hz","","50"]
["","Napon","","","V","","220-240"]