{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":8,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L3"]
[]
[]
[]
[]
["","","","","","RXS20L3V1B","RXS25L3V1B","RXS35L3V1B"]
["Razina tlaka zvuka","Grijanje","","Visoko","dBA","","","48"]
["","Hlađenje","","Visoko","dBA","","","48"]
["Standardna dodatna oprema","Priručnik za instalaciju","","","","","","1"]
["","Naljepnica punjenja radne tvari","","","","","","1"]
["","Višejezična naljepnica fluoriniranih stakleničkih plinova","","","","","","1"]
["","Drenažni priključak (samo modeli s dizalicom topline)","","","","","","1"]
["Refrigerant","Charge","","","TCO2Eq","","","2.5"]
["","GWP","","","","","","2,087.5"]
["","Punjenje","","","kg","","","1.2"]
["","Tip","","","","","","R-410A"]
["Motor ventilatora","Brzina","Hlađenje","Super nisko","o/min","","","780"]
["","","Grijanje","Super nisko","o/min","","","740"]
["Radno područje","Hlađenje","Ambijent:","Maks.","°CDB","","","46"]
["","","","Min.","°CDB","","","-10"]
["","Heating","Ambijent:","Maks.","°CWB","","","18"]
["","","","Min.","°CWB","","","-15"]
["Priključci cjevovoda","razlika u razini","IU - OU","Maks.","m","","","15"]
["","Punjenje dodatne radne tvari","","","kg/m","","","0,02 (za duljinu cjevovoda koja premašuje 10 m)"]
["Compressor","Tip","","","","","","Hermetički zabrtvljen kompresor s klatnom_"]
["Dimenzije","Uređaj","","Širina","mm","","","765"]
["","","","Dubina","mm","","","285"]
["","","","Visina","mm","","","550"]
["Težina","Uređaj","","","kg","","","34"]
["Ventilator","Količina zraka","Grijanje","Super nisko","cfm","","","904"]
["","","","Super nisko","m³/min","","","25.6"]
["","","Hlađenje","Super nisko","m³/min","","","30.1"]
["","","","Super nisko","cfm","","","1,063"]
["Power supply","Faza","","","","","","1~"]
["","Frekvencija","","","Hz","","","50"]
["","Napon","","","V","","","220-240"]
["Napomene","","","","","","","(1) - SL: tiha razina ventilatora za postavku stupnja protoka zraka"]
["Ventilator","Brzina protoka zraka","Hlađenje","Super nisko","m³/min","30.1","30.1"]
["","","Grijanje","Super nisko","m³/min","25.6","25.6"]
["","","","Super nisko","cfm","1063","1063"]
["","","Grijanje","Super nisko","cfm","904","904"]
["Dimenzije","Uređaj","","Visina","mm","550","550"]
["","","","Širina","mm","765","765"]
["","","","Dubina","mm","285","285"]
["Težina","Uređaj","","","kg","34","34"]
["Motor ventilatora","Brzina","Hlađenje","Super nisko","o/min","780","780"]
["","","Grijanje","Super nisko","o/min","740","740"]
["Kompresor","Tip","","","","Hermetički zabrtvljen kompresor s klatnom","Hermetički zabrtvljen kompresor s klatnom"]
["Raspon rada","Hlađenje","Ambijent:","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","46","46"]
["","Grijanje","Ambijent:","Min.","°CWB","-15","-15"]
["","","","Maks.","°CWB","18","18"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","46","46"]
["","Grijanje","","Visoko","dBA","47","47"]
["Radna tvar","Tip","","","","R-410A","R-410A"]
["","Punjenje","","","kg","1.0","1.0"]
["","Punjenje","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Priključci cjevovoda ","Duljina cjevovoda ","Maks. ","OU - IU","m","20","20"]
["Priključci cjevovoda","Punjenje dodatne radne tvari","","","kg/m","0,02 (za duljinu cjevovoda koja premašuje 10 m)","0,02 (za duljinu cjevovoda koja premašuje 10 m)"]
["","Razlika razine","IU - OU","Maks.","m","15","15"]
["Standardna dodatna oprema","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","Drain plug","","","","1"]
["Napajanje","Faza","","","","1~","1~"]
["","Frekvencija","","","Hz","50","50"]
["","Napon","","","V","220-240","220-240"]
["Napomene","","","","","(1) - 220 V"]
["","","","","","(2) - 230 V"]
["","","","","","(3) - 240 V"]
["Standardna dodatna oprema","Drain plug (only heat pump models)","","","","","1"]