{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":7,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-C"]
[]
[]
[]
[]
["","","","","","RZQ200C7Y1B","RZQ250C7Y1B"]
["Dimenzije","Uređaj","","Visina","mm","1,680"]
["","","","Širina","mm","930"]
["","","","Dubina","mm","765"]
["Težina","Uređaj","","","kg","183.0"]
["Compressor","Tip","","","","Hermetički zabrtvljen spiralni kompresor"]
["Radno područje","Hlađenje","Ambijent:","Min.","°CDB","-5.0"]
["","","","Maks.","°CDB","46.0"]
["","Heating","Ambijent:","Min.","°CWB","-15.0"]
["","","","Maks.","°CWB","15.0"]
["Razina zvučne snage","Hlađenje","","","dBA","78.0"]
["","Grijanje","","","dBA","78.0"]
["Radna tvar","Tip","","","","R-410A"]
["","Punjenje","","","kg","8.3"]
["","GWP","","","","2,087.5"]
["Priključci cjevovoda","Tekućina","","VP","mm","9.52"]
["","Plin","","VP","mm","22.2"]
["","Duljina cjevovoda","Maks.","OU - IU","m","100"]
["","","Sistem","Ne puni se","m","30"]
["Standardna dodatna oprema","Priručnik za instalaciju","","","","1"]
["","Spojne cijevi","","","","4"]
["Power supply","Faza","","","","3N~"]
["","Frekvencija","","","Hz","50"]
["","Napon","","","V","380-415"]
["Struja - 50 Hz","Preporučeni osigurač (MFA)","","","A","25"]
["Napomene","","","","","(1) - Unutarnja jedinica FDQ ima odvojeno napajanje"]
["","","","","","(2) - Vidi električne podatke na posebnim nacrtima"]
["Dimenzije","Uređaj","","Visina","mm","","1680"]
["","","","Širina","mm","","930"]
["","","","Dubina","mm","","765"]
["Težina","Uređaj","","","kg","","184.0"]
["Kompresor","Tip","","","","","Hermetički zabrtvljeni spiralni kompresor"]
["Raspon rada","Hlađenje","Ambijent:","Min.","°CDB","","-5.0"]
["","","","Maks.","°CDB","","46.0"]
["","Grijanje","Ambijent:","Min.","°CWB","","-15.0"]
["","","","Maks.","°CWB","","15.0"]
["Zvučna snaga","Hlađenje","","","dBA","","78.0"]
["","Grijanje","","","dBA","","78.0"]
["Radna tvar","Punjenje","","","kg","","9.3"]
["","GWP","","","","","2087.5"]
["","Punjenje","","","tCO2Eq","","19.4"]
["Priključci cjevovoda","Tekućina","","VP","mm","","12.70"]
["","Plin","","VP","mm","","22.2"]
["Priključci cjevovoda ","Duljina cjevovoda ","Maks. ","OU - IU","m","","100"]
["","","Sistem ","Ne puni se","m","","30"]
["Standardna dodatna oprema","Installation manual","","","","","1"]
["","Connection pipes","","","","","4"]
["Napajanje","Frekvencija","","","Hz","","50"]
["Struja - 50 Hz","Preporučeni osigurač (MFA)","","","A","","25"]