{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":96,"n_cols":9,"rows_kept":96,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-D"]
[]
[]
[]
[]
["","","","","","ACQ71DV1","ACQ100DV1","ACQ125DV1","ACQ140DV1"]
["Nivo zvučnog tlaka","Grijanje","","Visoko","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["","","","Tihi način rada","dBA","","36","","41"]
["","","","Nizak","dBA","","38","","43"]
["","Hlađenje","","Tihi način rada","dBA","","36","","41"]
["","","","Nizak","dBA","","38","","43"]
["","","","Visoko","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["Standardna dodatna oprema","Priručnik za instalaciju","","","","","Priručnik za instalaciju","","Priručnik za instalaciju"]
["","Radni priručnik","","","","","Radni priručnik","","Radni priručnik"]
["","Vijci","","","","","Vijci","","Vijci"]
["","Podloška","","","","","Podloška","","Podloška"]
["","Bežični daljinski upravljač","","","","","Bežični daljinski upravljač","","Bežični daljinski upravljač"]
["","Pokrivna rešetka na zaključavanje","","","","","Pokrivna rešetka na zaključavanje","","Pokrivna rešetka na zaključavanje"]
["","Baterija","","","","","Baterija","","Baterija"]
["Upravljački sustavi","Wired remote control","","","","","ARCWB","","ARCWB"]
["","Infrared remote control","","","","","ARCWLA","","ARCWLA"]
["Piping connections","Tekućina","","VP","mm","","9.52","","9.52"]
["","Plin","","VP","mm","","15.88","","15.88"]
["","Odvod vode","","","","","19.05","","19.05"]
["Ulazna snaga","Hlađenje","","Nom.","kW","","0.094","","0.137"]
["","Grijanje","","Nom.","kW","","0.094","","0.137"]
["Razina zvučne snage","Hlađenje","","","dBA","","56","","60"]
["","Grijanje","","","dBA","","56","","60"]
["Dimenzije","Jedinica","","Širina","mm","","820","","820"]
["","","","Dubina","mm","","820","","820"]
["","","","Visina","mm","","300","","300"]
["Kućište","Materijal","","","","","Galvanizirani čelik","","Galvanizirani čelik"]
["Težina","Uređaj","","","kg","","39","","39"]
["Ventilator","Količina zraka","Grijanje","Visoko","m³/min","","29.2","","34.0"]
["","","","Nizak","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","Hlađenje","Nizak","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","","Visoko","m³/min","","29.2","","34.0"]
["","","","Tihi način rada","m³/min","","17.6","","22.1"]
["","","Hlađenje","Tihi način rada","m³/min","","17.6","","22.1"]
["Dekorativni panel","Težina","","","kg","","4","","4"]
["","Dimenzije","","Visina","mm","","82","","82"]
["","","","Dubina","mm","","990","","990"]
["","","","Širina","mm","","990","","990"]
["","Boja","","","","","Bijelo","","Bijelo"]
["Power supply","Phase","","","","","1~","","1~"]
["","Naziv","","","","","V1","","V1"]
["","Frekvencija","","","Hz","","50","","50"]
["","Napon","","","V","","220-240","","220-240"]
["Ventilator","Količina zraka","Grijanje","Tihi način rada","m³/min","15","","22.1"]
["Ulazna struja","Grijanje","","Nom.","kW","0.067","","0.137"]
["","Hlađenje","","Nom.","kW","0.067","","0.137"]
["Ventilator","Količina zraka","Hlađenje","Tihi način rada","m³/min","15","","22.1"]
["Kućište","Materijal","","","","Galvanizirani čelik","","Galvanizirani čelik"]
["Dimenzije","Uređaj","","Visina","mm","265","","300"]
["","","","Širina","mm","820","","820"]
["","","","Dubina","mm","820","","820"]
["Težina","Uređaj","","","kg","31","","39"]
["Ventilator","Količina zraka","Hlađenje","Visoko","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","Nizak","m³/min","17.6","","26.3"]
["","","Grijanje","Visoko","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","Nizak","m³/min","17.6","","26.3"]
["Zvučna snaga","Hlađenje","","","dBA","54","","60"]
["","Grijanje","","","dBA","54","","60"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","Nizak","dBA","35","","43"]
["","","","Tihi način rada","dBA","32","","41"]
["","Grijanje","","Visoko","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","Nizak","dBA","35","","43"]
["","","","Tihi način rada","dBA","32","","41"]
["Priključci cjevovoda","Tekućina","","VP","mm","9.52","","9.52"]
["","Plin","","VP","mm","15.88","","15.88"]
["","Odvod vode","","","","19.05","","19.05"]
["Dekorativni panel","Dimenzije","","Visina","mm","82","","82"]
["","","","Širina","mm","990","","990"]
["","","","Dubina","mm","990","","990"]
["","Težina","","","kg","4","","4"]
["Upravljački sustavi","Infracrveno daljinsko upravljanje","","","","ARCWLA","","ARCWLA"]
["","Žično daljinsko upravljanje","","","","ARCWB","","ARCWB"]
["Standardna dodatna oprema","Installation manual","","","","Installation manual","","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","","Wireless remote control"]
["","Cover lock grill","","","","Cover lock grill","","Cover lock grill"]
["","Battery","","","","Battery","","Battery"]
["","Operation manual","","","","Operation manual","","Operation manual"]
["","Screws","","","","Screws","","Screws"]
["","Washer","","","","Washer","","Washer"]
["Napajanje","Faza","","","","1~","","1~"]
["","Frekvencija","","","Hz","50","","50"]
["","Napon","","","V","220-240","","220-240"]