{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-CB"]
[]
[]
[]
[]
["","","","","","CTXA15C2V1BB"]
["Ulazna struja","Hlađenje","","Nom.","kW","0.020"]
["","Grijanje","","Nom.","kW","0.020"]
["Kućište","Colour","","","","Crno"]
["Dimenzije","Uređaj","","Visina","mm","295"]
["","","","Širina","mm","798"]
["","","","Depth","mm","189"]
["Težina","Uređaj","","","kg","11.5"]
["Ventilator","Brzina protoka zraka","Cooling","Visoko","m³/min","11.0"]
["","","","Srednji","m³/min","8.2"]
["","","","Nizak","m³/min","6.1"]
["","","","Tihi način rada","m³/min","4.6"]
["","","Grijanje","Visoko","m³/min","10.9"]
["","","","Srednji","m³/min","8.7"]
["","","","Nizak","m³/min","6.4"]
["","","","Tihi način rada","m³/min","4.5"]
["Razina zvučne snage","Hlađenje","","","dBA","57"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","39"]
["","","","Srednji","dBA","32"]
["","","","Nizak","dBA","25"]
["","","","Tihi način rada","dBA","21"]
["","Grijanje","","Visoko","dBA","39"]
["","","","Srednji","dBA","32"]
["","","","Nizak","dBA","25"]
["","","","Tihi način rada","dBA","21"]
["Refrigerant","GWP","","","","675.0"]
["Priključci cjevovoda","Tekućina","","VP","mm","6.35"]
["","Plin","","VP","mm","9.50"]
["","Odvod vode","","","","18"]
["Upravljački sustavi","Infrared remote control","","","","ARC466A85"]
["","Wired remote control","","","","BRC073A1"]
["Standardna dodatna oprema","Priručnik za instalaciju","","","","1"]
["","Radni priručnik","","","","1"]
["","Zračni filtar","","","","2"]
["","Infracrveno daljinsko upravljanje","","","","1"]
["","Montažna ploča daljinskog kontrolnika","","","","1"]
["","Vreća s vijcima","","","","1"]
["","Poklopac vijka","","","","2"]
["","AAA suhe baterije","","","","2"]
["","Opće mjere sigurnosti","","","","1"]
["Power supply","Naziv","","","","V1"]
["","Phase","","","","1~"]
["","Frekvencija","","","Hz","50"]
["","Napon","","","V","220-240"]