{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9"]
["Razina tlaka zvuka","Grijanje","Visoko","dBA","38"]
["","","Srednji","dBA","36"]
["","","Nizak","dBA","30"]
["","Hlađenje","Srednji","dBA","36"]
["","","Nizak","dBA","30"]
["","","Visoko","dBA","38"]
["Standardna dodatna oprema","Priručnik za instalaciju","","","1"]
["","Radni priručnik","","","1"]
["","Izolacija priključka","","","1"]
["","Umetak za brtvljenje","","","1"]
["","Metalna stezaljka","","","1"]
["","Drenažno crijevo","","","1"]
["","Podloška za okvir vješalice","","","8"]
["","Materijal za brtvljenje","","","2"]
["","Stezaljke","","","6"]
["","Ploča za fiksiranje podloški","","","4"]
["","Vijci za prirubnice vodova","","","1"]
["","Zračni filtar","","","1"]
["Priključci cjevovoda","Tekućina","VP","mm","6.35"]
["","Plin","VP","mm","12.7"]
["","Odvod vode","","","VP20 (I.D. 20/O.D. 26)"]
["Ulazna struja","Hlađenje","Nom.","kW","0.060"]
["","Grijanje","Nom.","kW","0.060"]
["Sound power level","Hlađenje","","dBA","55"]
["","Grijanje","","dBA","55"]
["Dimenzije","Uređaj","Širina","mm","1,150"]
["","","Depth","mm","620"]
["","","Visina","mm","200"]
["Težina","Uređaj","","kg","30.0"]
["Fan","Vanjski statički tlak","Nom.","Pa","40"]
["Power supply","Phase","","","1~"]
["","Frekvencija","","Hz","50/60"]
["","Naziv","","","VE"]
["","Napon","","V","220-240"]
["Napomene","","","","(1) - Kada se spaja s vanjskom jedinicom za više sustava, pogledajte tehničke podatke vanjske jedinice za više sustava koju treba spojiti."]