{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":9,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A"]
[]
[]
[]
[]
["","","","","","FFA25A2VEB","FFA35A2VEB","FFA50A2VEB","FFA60A2VEB"]
["Kućište","Materijal","","","","Galvanizirana čelična ploča","Galvanizirana čelična ploča","Galvanizirana čelična ploča","Galvanizirana čelična ploča"]
["Dimenzije","Uređaj","","Visina","mm","260","260","260","260"]
["","","","Širina","mm","575","575","575","575"]
["","","","Dubina","mm","575","575","575","575"]
["Težina","Uređaj","","","kg","16.0","16.0","17.5","17.5"]
["Ventilator","Količina zraka","Hlađenje","Visoko","m³/min","9.0","10.0","12.0","14.5"]
["","Protok zraka","Hlađenje","Srednji","m³/min","8.0","8.5","10.0","12.5"]
["","","","Nizak","m³/min","6.5","6.5","7.5","9.5"]
["","","Grijanje","Visoko","m³/min","9.0","10.0","12.0","14.5"]
["","Protok zraka","Grijanje","Srednji","m³/min","8.0","8.5","10.0","12.5"]
["","","Grijanje","Nizak","m³/min","6.5","6.5","7.5","9.5"]
["Zvučna snaga","Hlađenje","","","dBA","48","51","56","60"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","31.0","34.0","39.0","43.0"]
["Razina zvučnog tlaka","Hlađenje","","Srednji","dBA","28.5","30.5","34.0","40.0"]
["Razina tlaka zvuka","Hlađenje","","Nizak","dBA","25.0","25.0","27.0","32.0"]
["","Grijanje","","Visoko","dBA","31.0","34.0","39.0","43.0"]
["Razina zvučnog tlaka","Grijanje","","Srednji","dBA","28.5","30.5","34.0","40.0"]
["Razina tlaka zvuka","Grijanje","","Nizak","dBA","25.0","25.0","27.0","32.0"]
["Priključci cjevovoda","Tekućina","","VP","mm","6.35","6.35","6.35","6.35"]
["","Plin","","VP","mm","9.52","9.52","12.70","12.70"]
["","Odvod vode","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Dekorativni panel","Model","","","","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W"]
["","Boja","","","","Bijelo (N9.5)","Bijelo (N9.5)","Bijelo (N9.5)","Bijelo (N9.5)"]
["","Dimenzije","","Visina","mm","46","46","46","46"]
["","","","Širina","mm","620","620","620","620"]
["","","","Dubina","mm","620","620","620","620"]
["","Težina","","","kg","2.8","2.8","2.8","2.8"]
["Ukrasna ploča 2","Model","","","","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S"]
["","Boja","","","","Srebrni","Srebrni","Srebrni","Srebrni"]
["","Dimenzije","","Visina","mm","46","46","46","46"]
["","","","Širina","mm","620","620","620","620"]
["","","","Dubina","mm","620","620","620","620"]
["","Težina","","","kg","2.8","2.8","2.8","2.8"]
["Ukrasna ploča 3","Model","","","","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1"]
["","Boja","","","","Bijelo (RAL9010)","Bijelo (RAL9010)","Bijelo (RAL9010)","Bijelo (RAL9010)"]
["","Dimenzije","","Visina","mm","55","55","55","55"]
["","","","Širina","mm","700","700","700","700"]
["","","","Dubina","mm","700","700","700","700"]
["","Težina","","","kg","2.7","2.7","2.7","2.7"]
["Ukrasna ploča 4","Model","","","","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1"]
["","Boja","","","","Bijelo (RAL9010)","Bijelo (RAL9010)","Bijelo (RAL9010)","Bijelo (RAL9010)"]
["","Dimenzije","","Visina","mm","55","55","55","55"]
["","","","Širina","mm","700","700","700","700"]
["","","","Dubina","mm","700","700","700","700"]
["","Težina","","","kg","2.7","2.7","2.7","2.7"]
["Upravljački sustavi","Infracrveno daljinsko upravljanje","","","","BRC7EB530 (standardna ploča), BRC7F530W (bijela ploča), BRC7F530S (siva ploča)","BRC7EB530 (standardna ploča), BRC7F530W (bijela ploča), BRC7F530S (siva ploča)","BRC7EB530 (standardna ploča), BRC7F530W (bijela ploča), BRC7F530S (siva ploča)","BRC7EB530 (standardna ploča), BRC7F530W (bijela ploča), BRC7F530S (siva ploča)"]
["","Žično daljinsko upravljanje","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Standardna dodatna oprema","Washer for hanger bracket","","","","8","8","8","8"]
["","Thermal insulation tube","","","","2","2","2","2"]
["","Hose band","","","","1","1","1","1"]
["","Drain hose","","","","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1"]
["","Screws","","","","4","4","4","4"]
["","Sealing material","","","","4","4","4","4"]
["","Tie-wraps","","","","7","7","7","7"]
["Napajanje","Faza","","","","1~","1~","1~","1~"]
["","Frekvencija","","","Hz","50","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240","220-240"]